anologRead : 10 bit

analogWrite : 8 bit